Placing the Rotor on the Centrifuge
Warning: If the pins of the rotor are not properly aligned on the centrifuge before running, damage can result!
1. Turn rotor upside down and note the location/orientation of its pins.
2. The pins on the rotor should be positioned parallel to the pins of the centrifuge drive shaft. (i.e The pins should touch at both points and not be in-between the drive shaft pins-See Drawing Below)
Black lines/dots  represent the drive shaft, red lines/dots are  rotor pins
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3. Lower the rotor carefully on the Drive shaft, with its pins in the correct orientation.
4. Once lowered, check to make sure the rotor pins are hugging the drive shaft pins before tightening the rotor and running the centrifuge.
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